Steps for choosing airfoil:

1.The first step in airfoil selection is to determine the design lift coefficient of the airfoil.

The design lift is the aircraft lift at the most fuel intensive segment of the aircraft mission, i.e. The flight condition at which the aircraft is supposed to fly most of the time







